

Touchdown point ≈ 45° behind

Turn Base Leg

30° Bank

Wind

45°

At 1000’ AGL

Power 2000-2100 RPM

Trim to hold altitude

Airspeed ≈ 100 MPH

25R

7L

Flaps 25°

Pitch for 80 MPH

Power 1500 RPM

RPM +- 200 for altitude

Flaps 40°

Pitch for 75 MPH

Power 1500 RPM

RPM +- 200 for altitude

Abeam touchdown point

Power to 1500 RPM

Flaps 10°

Pitch for 85 MPH

At ½ mile offset to runway centerline

Turn Downwind Leg

30° Bank

At 500’ AGL

Turn crosswind leg

30° Bank

Departure Leg

Full Power

Pitch for Vy – 87 MPH

Track along runway extended centerline

Lined up on centerline

Turn Final

30° Bank